{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Inquiry","SX"],"not_rendered":{"charts":0,"images":2,"macros":1,"external_links":0,"defined_names":8,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Inquiry","index":0,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":false,"merged":[[2,4,2,5],[3,4,3,5]]}
[null,"PCR","Inquiry Form",null,{"$f":"IF(C6>0,TODAY(),\"\")","v":""}]
[null,null,"Send your request for offer usign this form",null,null,"SEND MAIL"]
[null,"Company:",null,"Email:"]
[]
[null,"No.","PIPE Standard ","PIPE dimension","Gasket","QTY."]
[null,{"$f":"IF(C6>0,\"1\",\"\")","v":""}]
[null,{"$f":"IF(C7>0,\"2\",\"\")","v":""}]
[null,{"$f":"IF(C8>0,\"3\",\"\")","v":""}]
[null,{"$f":"IF(C9>0,\"4\",\"\")","v":""}]
[null,{"$f":"IF(C10>0,\"5\",\"\")","v":""}]
[null,{"$f":"IF(C11>0,\"6\",\"\")","v":""}]
[null,{"$f":"IF(C12>0,\"7\",\"\")","v":""}]
[null,{"$f":"IF(C13>0,\"8\",\"\")","v":""}]
[null,{"$f":"IF(C14>0,\"9\",\"\")","v":""}]
[null,{"$f":"IF(C15>0,\"10\",\"\")","v":""}]
[null,{"$f":"IF(C16>0,\"11\",\"\")","v":""}]
[null,{"$f":"IF(C17>0,\"12\",\"\")","v":""}]
[null,{"$f":"IF(C18>0,\"13\",\"\")","v":""}]
[null,{"$f":"IF(C19>0,\"14\",\"\")","v":""}]
[null,{"$f":"IF(C20>0,\"15\",\"\")","v":""}]
[null,{"$f":"IF(C21>0,\"16\",\"\")","v":""}]
[null,{"$f":"IF(C22>0,\"17\",\"\")","v":""}]
[null,{"$f":"IF(C23>0,\"18\",\"\")","v":""}]
[null,{"$f":"IF(C24>0,\"19\",\"\")","v":""}]

{"sheet":"SX","index":1,"n_rows":15,"n_cols":7,"rows_kept":15,"cut":false,"hidden":true,"merged":[]}
["COLOR","DIN_11850R2","ISO_1127","ASTM_270","DIN_1850R1","SMS_3008","Pipe_OD"]
["EPDM blue","DN10    /   Ø13","06   /    Ø10,2","1/8\"   /    Ø3,18","DN04   /    Ø6","1\"   /    Ø25","Ø 14"]
["EPDM white","DN15    /   Ø19","08   /    Ø13,5","1/4\"   /    Ø6,35","DN06   /    Ø8","1\"1/4   /    Ø32","Ø 24"]
["EPDM gray","DN20    /   Ø23","10   /    Ø17,2","3/8\"   /    Ø9,53","DN08   /    Ø10","1\"1/2   /    Ø38","Ø 30"]
["EPDM black EC","DN25    /   Ø29","15   /    Ø21,3","1/2\"   /    Ø12,7","DN10   /    Ø12","2\"   /    Ø51","Ø 42"]
["Silikon red HT","DN32    /   Ø35","20   /    Ø26,9","3/4\"   /    Ø19,05","DN15   /    Ø18","2\"1/2   /    Ø63,5"]
["Silikon purple","DN40    /   Ø41","25   /    Ø33,7","1\"   /    Ø25,4","DN20   /    Ø22","3\"   /    Ø76,1"]
[null,"DN50    /   Ø53","32   /    Ø42,4","1''1/2   /    Ø38,1","DN25   /    Ø28","4\"   /    Ø101,6"]
[null,"DN65    /   Ø70","40   /    Ø48,3","2\"   /    Ø50,8","DN32   /    Ø34"]
[null,"DN80    /   Ø85","50   /    Ø60,3","2''1/2   /    Ø63,5","DN40   /    Ø40"]
[null,"DN100    /   Ø104","65   /    Ø76,1","3\"   /    Ø76,2","DN50   /    Ø52"]
[null,"DN125    /   Ø129","80   /    Ø88,9","4\"   /    Ø101,6"]
[null,"DN150    /   Ø154","100   /    Ø114,3","6\"   /    Ø152,4"]
[null,"DN200    /   Ø204","125   /    Ø139,7","8\"   /    Ø203,2"]
[null,null,"150   /    Ø168,3"]